1. Why can you only use certain pins for analogWrite()?

Because only certain pins on different Arduino boards have frequency that are compatible with the analogWrite feature.

1. What is the range the map() function maps the value to? Why this range?

Negative -1023 to 1023? (I’m not sure because the reference is kind of confusing…)